**PROGRESSIVE COLLAPSE ANALYSIS**

**OF**

**THIN-PLATED STRUCTURES**

**USING ISUM**

A dissertation

presented to

the faculty of

Department of Civil and Environmental Engineering

Delhi Technological University-Delhi



In Partial Fulfilment

of the Requirements for the Degree

Master of Technology

By

YOGESH KUMAR JANGID

Dr. S.K. Panda and Dr. A.K. Gupta, Dissertation Supervisors

JULY-2013

**CERTIFICATE**

The undersigned have examined the dissertation entitled

**PROGRESSIVE COLLAPSE ANALYSIS**

**OF**

**THIN-PLATED STRUCTURES**

**USING ISUM**

presented by Yogesh Kumar Jangid

a candidate for Master of Technology

and hereby certify that in their opinion it is worthy of acceptance

Dr. S.K. Panda

Dr. A.K. Gupta

**DECLARATION**

I Certify that

1. The work contained in this thesis is original and has been done by me under the guidance of my supervisor.
2. The work has not been submitted to any other Institute for any degree or diploma.
3. I have followed the guidelines provided by the University in preparing the thesis.
4. I have conformed to the norms and guidelines given in the Ethical Code of Conduct of the Institute.
5. Whenever I have used materials (data, theoretical analysis, figures, and text) from other sources, I have given due credit to them by citing them in the text of the thesis and giving their details in the references.

Yogesh Kumar Jangid

(2K11/STE/19)

Department of Civil and Environmental Engineering

Delhi Technological University, Delhi

**ACKNOWLEDGEMENT**

I would like to sincerely and wholeheartedly thank my advisor Dr. S.K. Panda and Dr. A.K. Gupta for their close guidance, kindness, encouragements, patience, and supervision throughout various stages of the dissertation. Without their help and encouragement, this dissertation would not be possible.

I wish to convey my sincere gratitude to Prof. A.K. Gupta (former H.O.D) and Prof. A. Trivedi (H.O.D.), and all the faculties of Civil Engineering Department, Delhi Technological University who have enlightened me during my project.

Most importantly, I would like thank my parents, for their unconditional support, love, and affection. Their encouragement and endless love made everything easier to achieve.

TABLE OF CONTENTS

TITLEi

CERTIFICATEii

DECLARATIONiii

ACKNOLEDGEMENTiv

TABLE OF CONTENTSv

LIST OF FIGURESvii

ABSTRACTix

Chapter 1 Introduction1

1.1 Idealized structural unit method1

1.2 ISUM vs. FEM2

1.3 Progressive collapse analysis 3

1.7.1 Introduction3

1.7.2 Mechanism of progressive collapse analysis4

1.5 Objectives 6

Chapter 2 Literature review7

Chapter 3 Mathematical formulation10

3.1 Introduction10

3.2.1 Effective width concept10

3.2.2 Tangent modulus12

3.2.1 Secant modulus13

3.1 Progressive collapse analysis: SUM13

3.3 Problem statement19

3.2.1 A short box column with L=500 mm21

3.2.1 A medium box column with L=8000 mm22

3.2.1 A long box column with L=21000 mm24

Chapter 4 Results and discussions25

3.2.1 A short box column with L=500 mm25

3.2.1 A medium box column with L=8000 mm27

3.2.1 A long box column with L=21000 mm30

**Conclusions36**

**References37**

**LIST OF FIGURES**

1. House of cards effect………………………………………………………………………4
2. Actual Stress Distribution in a Compressed Stiffened Plate……………………………..11
3. Stress-strain curve ………………………………………………………………………12
4. Secant modulus ……………………………………………..…………………………..13
5. The local coordinate system for the ISUM plate element with its nodal forces and dis-placements …………………………………………………………………………….…14
6. A schematic of the failure behavior considered for developing the present ISUM plate element …………………………………………………………………………………..15
7. Structural models used for (a) ANSYS nonlinear FEA and (b) ISUM of one bay (short) box column ………………………………………………………………………………20
8. Structural models used for (a) ANSYS nonlinear FEA and (b) ISUM of the medium box column with L =8000 mm …………………..…………………………………………...23
9. Deformed shape and von Mises stress distribution of the short box with L=500 mm at ultimate limit state as obtained by FEA (ANSYS) ………………………………...……25
10. The progressive collapse behavior in terms of axial compressive load versus edge shortening curves for the short box column with L =500 mm, as obtained by nonlinear FEA and ISUM…………………………………………………………………………..26
11. The progressive collapse behavior in terms of axial compressive load versus edge shortening curves for the medium box column with L = 8000 mm, as obtained by nonlinear FEA and ISUM………………………………………………………………...27
12. Deformed shape and von Mises stress distribution of the medium box column with L=8000mm at ultimate limit state (shown for a quarter of the structure), obtained by ANSYS nonlinear FEA…………………………………………………………………..29
13. The progressive collapse behavior in terms of axial compressive load versus edge shortening curves for the medium box column with L=21000 mm, as obtained by nonlinear FEA and ISUM………………………………………………………………...30
14. Average stress versus strain curves for a plate element of compressed upper-flange of the medium box column (with L=8000mm) at center and at end………………………32....33
15. Deformed shape and von Mises stress distribution of the long box column with L =21,000mm at ultimate limit state (shown for a quarter of the structure), as obtained by ANSYS nonlinear FEA…………………………………………………………………..35

**ABSTRACT**

Box columns are often used as main strength members of various types of thin-plated structures such as ships, ship-shaped offshore structures, and aerospace structures. Until and after the ultimate limit state is reached, box columns exhibit highly nonlinear structural behaviour in terms of geometrical and material aspects. In particular, the effects of local buckling, global buckling, and their interaction play a significant role in the resulting consequences of box columns under extreme actions. In order to calculate the maximum load carrying capacity of box columns, it is thus highly required to perform the progressive collapse analysis to take into account progressive failures of individual components and their interacting effects.

The aim of the present study is to investigate the applicability of ISUM to the progressive collapse analysis of box columns which are typical examples of main strength members in land-based structures. Theoretical outline of the method is addressed. Short, medium and long box columns in length are studied in terms of interacting effects between local component failure modes and global system failure modes. A comparison of ISUM with more refined nonlinear finite element method (FEM) computations is also made.